**APM 2 Lights**

|  |  |
| --- | --- |
| Power | On when powered |
| A (red) | **Solid** = armed, motors will spin when throttle raised  **Single Blink** = motor disarmed  **Double Blink** = motor disarmed, cannot arm  because of failure in pre-arm checks |
| B (yellow) | Only flashes along with A and B during calibration or as part of the in-flight auto trim feature |
| C (blue) | **Solid** = GPS working, 3D lock  **Blinking** = GPS working, no lock  **OFF** = GPS not attached or not working |
| PPM/Serial | Flashing when data detected |

**GPS Lights**

|  |  |
| --- | --- |
| Power | Solid red when powered |
| GPS lock | Flashing blue when 3D GPS lock acquired |